Jump to main content

##

# 2.32.21 DMAC_ERROR Enum

## C

    typedef enum
    {
        /* Data was transferred successfully. */
        DMAC_ERROR_NONE

        /* DMA address error. */
        DMAC_ERROR_ADDRESS_ERROR

    } DMAC_ERROR;

## Summary

Identifies the available DMA operating modes.

## Description

This data type Identifies if a transfer had an address error or not.

## Remarks

The identification of an error transaction takes place in the DMA ISR.