Jump to main content

##

# 2.18.11 CMPx_DACDataLowWrite Function

## C

    // x is the instance number of the CMP peripheral
    inline static void CMPx_DACDataLowWrite(uint16_t dacLowLimit);

## Summary

Sets the lower limit of slope .

## Description

This inline function writes lower limit of the slope.

## Precondition

None.

## Parameters

Param | Description
dacLowLimit | lower limit of slope

## Returns

None.

## Example

    CMP1_DACDataLowWrite(0xCD);

## Remarks

Available only in slope mode.