Jump to main content

##

# 2.39.14 ECIA_InterruptEnable Function

## C

    void ECIA_InterruptEnable(ECIA_INT_SOURCE int_src)

## Summary

Enables interrupt at both ECIA and NVIC level for the given interrupt source.

## Description

Enables interrupt at both ECIA and NVIC level. This API enables the interrupt source, corresponding block interrupt and the corresponding direct or aggregate NVIC interrupt.

## Precondition

None.

## Parameters

Param | Description
--- | ---
int_src | One of the interrupt source from the enum ECIA_INT_SOURCE

## Returns

None

## Example

    ECIA_InterruptEnable(ECIA_AGG_INT_SRC_GPIO002);

## Remarks

None