Jump to main content

##

# 2.51.26 GPIO_PinGroupOutputConfig Function

## C

    void GPIO_PinGroupOutputConfig(GPIO_PIN pin, GPIO_ALT_OUT altOutputEn)

## Summary

Either enables or disables control of the GPIO pin using the Group output register

## Description

Every GPIO has two mechanisms to set a GPIO data output - either using the grouped GPIO output register or using the single GPIO output data bit located in the Pin Control register. This API lets application enable either of the two mechanisms based on the GPIO_ALT_OUT enum value.

## Precondition

None.

## Parameters

Param | Description
--- | ---
pin | One of the GPIO pins from the enum GPIO_PIN
altOutputEn | One of the values from the enum GPIO_ALT_OUT

## Returns

None

## Example

    GPIO_PinGroupOutputConfig(GPIO_PIN_GPIO012, GPIO_ALT_OUT_DIS);

## Remarks

None