Jump to main content

##

# 2.120.2.27 TCx_CHy_CaptureStop Function

## C

    /* x = TC instance number, y= channel number */
    void TCx_CHy_CaptureStop ( void );

## Summary

Stops the given TC channel counter.

## Description

This function stops the clock and thus counter of associated channel, preventing it from capturing signal-event counter values.

## Precondition

TCx_CHy_CaptureInitialize() function must have been called first for the given channel.

## Parameters

None

## Returns

None.

## Example

    TC0_CH1_CaptureInitialize();
    TC0_CH1_CaptureStart();
    // Capture signal event counter values.
    TC0_CH1_CaptureStop();

## Remarks

None