Jump to main content

##

# 2.65.12 MCPWM_ChannelSecondaryTriggerSet Function

## C

    void MCPWM_ChannelSecondaryTriggerSet (MCPWM_CH_NUM channel, uint16_t trigger)

## Summary

Writes the secondary trigger compare value to trigger ADC conversion

## Description

This function writes secondary trigger compare value to trigger ADC conversion

## Precondition

MCPWM_Initialize() function must have been called first for the associated instance and associated channel must be running.

## Parameters

Param | Description
--- | ---
channel | MCPWM channel number
trigger | compare value which is compared with time base

## Returns

None

## Example

    MCPWM_Initialize();
    MCPWM_Start();
    MCPWM_ChannelSecondaryTriggerSet(MCPWM_CH_0, 0x25);

## Remarks

When trigger compare value matches the counter, interrupt can be generated and this trigger is used to synchronize an ADC conversion with the PWM.