Jump to main content

##

# 2.133.20 XDMAC_DESCRIPTOR_VIEW_2 Struct

## C

        typedef struct {

            /* Next Descriptor Address number. */
            uint32_t mbr_nda;

            /* Micro-block Control Member. */
            XDMAC_MICRO_BLOCK_CONTROL mbr_ubc;

            /* Source Address Member. */
            uint32_t mbr_sa;

            /* Destination Address Member. */
            uint32_t mbr_da;

            /* Configuration Register. */
            /* TODO: Redefine type to XDMAC_CC white updating to N type */
            uint32_t mbr_cfg;

        } XDMAC_DESCRIPTOR_VIEW_2;

## Summary

Defines the descriptor view 2 available for master transfer.

## Description

This data type defines the descriptor view 2 .

## Remarks

This feature may not be available on all devices. Refer to the specific device data sheet to determine availability.