Jump to main content

##

# 2.61.38 LCDCx_SetHSYNCPulseWidth Function

## C

    // x - Instance of the LCDC peripheral

    void LCDCx_SetHSYNCPulseWidth(uint16_t value)

## Summary

Sets HSYNC pulse length, given in pixel clock cycles

## Description

None

## Precondition

None.

## Parameters

Param | Description
--- | ---
value | the 16-bit pulse width, must be greater than 1

## Returns

None

## Remarks

None