Jump to main content

##

# 3.24.17 Real-Time Clock and Calendar(RTCC)

The RTCC peripheral is useful in applications which requires clock and calendar features.

## Using The Library

RTCC Peripheral library provides API's that can be used to perform below functionalities on the RTCC peripheral.

- Initialize the RTCC

- Read and write the time and date registers.

- Set alarm time and date.

- Enable/Disable the RTCC interrupt.

- Register a callback.

## Library Interface

RTCC peripheral library provides the following interfaces:

Functions

Name | Description
--- | ---
RTCC_Initialize | Initialize the RTCC peripheral
RTCC_TimeSet | Sets time and date in the RTCC peripheral
RTCC_TimeGet | Gets time and date from the RTCC peripheral
RTCC_AlarmSet | Sets the alarm time and date in the RTCC peripheral
RTCC_CallbackRegister | Registers the function to be called from interrupt
RTCC_InterruptEnable | Enables RTCC peripheral interrupt
RTCC_InterruptDisable | Disables RTCC peripheral interrupt

Data types and constants

Name | Type | Description
--- | --- | ---
RTC_ALARM_MASK | Enum | Possible options for recurrence of RTCC alarm
RTC_INT_MASK | Enum | Mask for enabling and disabling the RTCC interrupt
RTC_CALLBACK | Typedef | Defines the data type and function signature of the Real Time Clock Calendar callback function