Jump to main content

##

# 2.15.52 CLOCK_FAIL_STATUS_MASKS Enum

## C

    typedef enum
    {
        CLOCK_GEN1_FAIL_MASK = 0x1,
        CLOCK_GEN2_FAIL_MASK = 0x2,
        CLOCK_GEN3_FAIL_MASK = 0x4,
        CLOCK_GEN4_FAIL_MASK = 0x8,
        CLOCK_GEN5_FAIL_MASK = 0x10,
        CLOCK_GEN6_FAIL_MASK = 0x20,
        CLOCK_GEN7_FAIL_MASK = 0x40,
        CLOCK_GEN8_FAIL_MASK = 0x80,
        CLOCK_GEN9_FAIL_MASK = 0x100,
        CLOCK_GEN10_FAIL_MASK = 0x200,
        CLOCK_GEN11_FAIL_MASK = 0x400,
        CLOCK_GEN12_FAIL_MASK = 0x800,
        CLOCK_GEN13_FAIL_MASK = 0x1000,
        CLOCK_PLL1_FAIL_MASK = 0x1000000,
        CLOCK_PLL2_FAIL_MASK = 0x2000000,
    } CLOCK_FAIL_STATUS_MASKS;

## Summary

Defines the fail status mask for each PLL generator and Clock generator.

## Description

This enumeration defines the maks to be used on return value of CLOCK_FailStatusGet to know individual clock failure status.

## Remarks

None.