Jump to main content

##

# 2.99.25 RTC_Timer32InterruptDisable Function

## C

    void RTC_Timer32InterruptDisable (RTC_TIMER32_INT_MASK interrupt)

## Summary

Disable selected RTC interrupt

## Description

This function allows the application to disable period match, compare match and periodic event interrupt

## Precondition

RTC_Initialize must have been called for the associated RTC instance. The Interrupt option in MCC should have been enabled. The RTC peripheral should have been configured for 32-bit timer counter operation. A valid event handling callback function should have been registered by calling the RTC_Timer32CallbackRegister() function.

## Parameters

Param | Description
--- | ---
InterruptMask | Specifies interrupt source to be disabled

## Returns

None.

## Example

    RTC_Timer16InterruptDisable(RTC_TIMER16_INT_MASK_PERIOD_MATCH);

## Remarks

None.