Jump to main content

##

# 2.87.9 POWER_DS_ExtendedSemaphoreEnable Function

## C

void POWER_DS_ExtendedSemaphoreEnable(void);

## Summary

Enables the general purpose register retention in the Deep Sleep mode

## Description

Enables the general purpose register retention in the Deep Sleep mode

## Precondition

None.

## Parameters

None.

## Returns

None.

## Example

POWER_DS_ExtendedSemaphoreEnable()

## Remarks

This function is only available for the devices which has deep sleep controller. MCC will generate this function only for the selected devices accordingly. Check device datasheet for more information.