Jump to main content

##

# 2.8.23 CAN_TX_EVENT_FIFO Struct

## C

    typedef struct
    {
        /* Identifier */
        uint32_t id:29;
        /* Remote Transmission Request */
        uint32_t rtr:1;
        /* Extended Identifier */
        uint32_t xtd:1;
        /* Error State Indicator */
        uint32_t esi:1;

        /* Tx Timestamp */
        uint32_t txts:16;
        /* Data Length Code */
        uint32_t dlc:4;
        /* Bit Rate Switch */
        uint32_t brs:1;
        /* FD Format */
        uint32_t fdf:1;
        /* Event Type */
        uint32_t et:2;
        /* Message Marker */
        uint32_t mm:8;

    } CAN_TX_EVENT_FIFO;

## Summary

CAN Tx Event FIFO Element Structure.

## Description

This data structure defines CAN Tx Event FIFO Element.

## Remarks

None.