Jump to main content

##

# 2.6.2 AIC_INT_IrqEnable Function

## C

    void AIC_INT_IrqEnable ( void )

## Summary

Enable interrupt to the processor.

## Description

AIC will generate interrupts to the processor when an interrupt condition is met.

## Precondition

AIC should be initialized with a call to AIC_Initialize() function.

## Parameters

None.

## Returns

None.

## Example

    AIC_INT_IrqEnable ( );

## Remarks

None.