Jump to main content

##

# 2.80.13 PDECx_HALLPatternSet Function

## C

    bool PDECx_HALLPatternSet ( uint8_t pattern ) // x is instance of the peripheral and it is applicable only for devices having multiple instances of the peripheral.

## Summary

Writes the hall pattern.

## Description

This function writes the hall pattern in CC0 LSB.

## Precondition

PDECx_HALLInitialize function must have been called first for the given channel.

## Parameters

Param | Description
--- | ---
pattern | hall pattern

## Returns

true - If hall pattern set false - If hall pattern is not set

## Example

    uint8_t position;

    PDEC_HALLInitialize();
    PDEC_HALLStart();
    PDEC_HALLPatternSet(0x3);

## Remarks

None