Jump to main content

##

# 2.3.20 ADC_ChannelSamplingStart Function

## C

    ADC_ChannelSamplingStart(void)

## Summary

Enables the Analog Mux Input and starts sampling on the ADC core and channel that was specified using the ADC_SoftwareControlledConversionEnable() API

## Description

Enables the Analog Mux Input and starts sampling. This API must be used in conjuction with ADC_SoftwareControlledConversionEnable() API to start the conversion on the given channel.

## Precondition

ADCx_Initialize() function must have been called first for the associated instance.

## Parameters

None

## Returns

None

## Example

    ADC_ChannelSamplingStart();

## Remarks

None