Jump to main content

##

# 2.130.15 UARTx_WriteByte Function

## C

    /* x = UART instance number */

    /* Blocking mode */

    void UARTx_WriteByte( int data )

## Summary

Submits a byte of data to the given UART peripheral to transfer

## Description

This function submits a byte of data to the UART peripheral to transfer. This Function is available only in non-interrupt mode.

## Precondition

UARTx_Initialize must have been called for the associated UART instance.

## Parameters

Param | Description
--- | ---
data | Data byte to be transferred

## Returns

None

## Example

    char myData = 'A';

    UART1_WriteByte(myData);

## Remarks

None