Jump to main content

##

# 2.80.25 PDECx_COUNTERStatusGet Function

## C

    PDEC_COUNTER_STATUS PDECx_COUNTERStatusGet (void) // x is instance of the peripheral and it is applicable only for devices having multiple instances of the peripheral.

## Summary

Identifies status of the counter mode interrupts

## Description

This function returns the status of the interrupts that occur in counter mode.

## Precondition

PDECx_COUNTERInitialize must have been called first.

## Parameters

None

## Returns

PDEC_COUNTER_STATUS - status of the counter interrupts

## Example

    PDEC_COUNTER_STATUS status;
    status = PDEC_COUNTERStatusGet();

## Remarks

None