Jump to main content

##

# 2.41.13 EFC_ERROR Enum

## C

    typedef enum
    {
        /* No Error Occured */
        EFC_ERROR_NONE = 0x1,
        /*In-valid command*/
        EFC_CMD_ERROR = 0x2,
        /*Flash region is locked*/
        EFC_LOCK_ERROR = 0x4,
        /*Flash Error*/
        EFC_FLERR_ERROR = 0x8,
        /*Flash Encountered an ECC error*/
        EFC_ECC_ERROR = 0xF0000,
    } EFC_ERROR;

## Summary

Defines the data type for the EFC Error.

## Description

This enum is used to define error encountered during last Flash operation.

## Remarks

None.