Jump to main content

##

# 2.120.2.39 TC_CAPTURE_STATUS Enum

## C

    typedef enum
    {
        TC_CAPTURE_NONE = 0U,
        TC_CAPTURE_COUNTER_OVERFLOW = TC_SR_COVFS_Msk,
        TC_CAPTURE_LOAD_OVERRUN = TC_SR_LOVRS_Msk,
        TC_CAPTURE_A_LOAD = TC_SR_LDRAS_Msk,
        TC_CAPTURE_B_LOAD = TC_SR_LDRBS_Msk,
        TC_CAPTURE_STATUS_MSK = TC_SR_COVFS_Msk | TC_SR_LOVRS_Msk | TC_SR_LDRAS_Msk | TC_SR_LDRBS_Msk,
        TC_CAPTURE_STATUS_INVALID = 0xFFFFFFFF
    }TC_CAPTURE_STATUS;

## Summary

Identifies channel interrupt source mask

## Description

This enumeration identifies TC capture mode interrupt source mask.

## Remarks

None.