Jump to main content

##

# 2.61.57 LCDCx_SetVerticalBackPorchWidth Function

## C

    // x - Instance of the LCDC peripheral

    void LCDCx_SetVerticalBackPorchWidth(uint16_t value)

## Summary

Sets VSYNC back porch width, give in number of lines

## Description

This field indicates the number of lines at the beginning of the frame

## Precondition

None.

## Parameters

Param | Description
--- | ---
value | the 16-bit porch width, must be greater than 1

## Returns

None

## Remarks

None