Jump to main content

##

# 2.47.68 FLEXCOMx_TWI_NACKDataPhase Function

## C

    /* x = FLEXCOM instance number */

    /* TWI slave mode */

    void FLEXCOMx_TWI_NACKDataPhase(bool isNACKEnable)

## Summary

Configures the hardware to send ACK or NAK for the next byte that will be received from the TWI master

## Description

This function lets the application send ACK or NAK for the next data from the I2C master

## Precondition

FLEXCOMx_TWI_Initialize must have been called for the associated FLEXCOM TWI instance.

## Parameters

Param | Description
--- | ---
true | Send NAK to the next data from I2C master
false | Send ACK to the next data from I2C master

## Returns

None

## Example

    // Send NAK for the next data from I2C master
    FLEXCOM0_TWI_NACKDataPhase(true);

## Remarks

None