Jump to main content

##

# 2.120.1.54 TCx_Capture8bitChannel0Get Function

## C

    /* x = TC instance number */
    uint8_t TCx_Capture8bitChannel0Get( void );

## Summary

Reads capture value from channel 0.

## Description

This function reads the captured value stored in CC[0]. Value can be read from interrupt routine or by polling.

## Precondition

TCx_CaptureInitialize() function must have been called first.

## Parameters

None.

## Returns

Captured value from channel 0.

## Example

    uint8_t captureValue = 0;
    TC0_CaptureInitialize();
    TC0_CaptureStart();
    captureValue = TC0_Capture8bitChannel0Get();

## Remarks

None.