Jump to main content

##

# 2.3.12 ADCx_InterruptsDisable Function

## C

    void ADCx_InterruptsDisable(ADC_STATUS interruptMask); // x is instance of the peripheral and it is applicable only for devices having multiple instances of the peripheral.

## Summary

This function disables the interrupts.

## Description

This function disables the multiple interrupts.

## Precondition

ADCx_Initialize() function must have been called first for the associated instance.

## Parameters

Param | Description
--- | ---
interruptMask | interrupt flags to be disbaled

## Returns

None

## Example

    ADC0_Initialize();
    ADC0_InterruptsDisable(ADC_STATUS_RESRDY);

## Remarks

None