Jump to main content

##

# 2.8.13 CAN_MSG_RAM_CONFIG Struct

## C

    typedef struct
    {
        /* Rx FIFO0 base address */
        can_rxf0e_registers_t *rxFIFO0Address;

        /* Rx FIFO1 base address */
        can_rxf1e_registers_t *rxFIFO1Address;

        /* Rx Buffer base address */
        can_rxbe_registers_t *rxBuffersAddress;

        /* Tx Buffers/FIFO base address */
        can_txbe_registers_t *txBuffersAddress;

        /* Tx Event FIFO base address */
        can_txefe_registers_t *txEventFIFOAddress;

        /* Standard Message ID Filter base address */
        can_sidfe_registers_t *stdMsgIDFilterAddress;

        /* Extended Message ID Filter base address */
        can_xidfe_registers_t *extMsgIDFilterAddress;
    } CAN_MSG_RAM_CONFIG;

## Summary

CAN Message RAM Configuration structure.

## Description

This data structure defines the CAN Message RAM Base address for Rx FIFO0, Rx FIFO1, Rx Buffers, Tx Buffers/FIFO, Tx Event FIFO, Standard Message ID Filter and Extended Message ID Filter configuration.

## Remarks

None.