Jump to main content

##

# 2.112.30 I2CSMBx_TargetStart Function

## C

    /* x = I2C SMBUS peripheral instance number */

    /* I2C SMBUS Target mode */

    void I2CSMBx_TargetStart(void)

## Summary

Configures the DMA and starts the target in receive mode

## Description

Configures the DMA and starts the target in receive mode

## Precondition

I2CSMBx_Initialize must have been called for the associated I2C instance.

## Parameters

None.

## Returns

None

## Example

    I2CSMB0_TargetStart();

## Remarks

None.