Jump to main content

##

# 2.61.76 LCDCx_INTERRUPT Enum

## C

    // x - Instance of the LCDC peripheral

    typedef enum
    {
        LCDCx_INTERRUPT_SOF,
        LCDCx_INTERRUPT_DIS,
        LCDCx_INTERRUPT_DISP,
        LCDCx_INTERRUPT_FIFOERR,
        LCDCx_INTERRUPT_BASE,
        LCDCx_INTERRUPT_OVR1,
        LCDCx_INTERRUPT_OVR2,
        LCDCx_INTERRUPT_HEO,
        LCDCx_INTERRUPT_PP,
    } LCDCx_INTERRUPT;

## Summary

Defines the interrupts generated by the controller

## Description

## Remarks

None.