Jump to main content

##

# 2.109.24 SENT_TRANSMIT_STATUS Enum

## C

    typedef enum
    {
        SENT_TRANSMIT_SYNCTXEN = 0x1,      /**< Synchronization Period Status Transmit Enable bit */
        SENT_TRANSMIT_NIBBLE1 = 0x10,      /**< Module is transmitting Data Nibble 1 */
        SENT_TRANSMIT_NIBBLE2 = 0x20,      /**< Module is transmitting Data Nibble 2 */
        SENT_TRANSMIT_NIBBLE3 = 0x30,      /**< Module is transmitting Data Nibble 3 */
        SENT_TRANSMIT_NIBBLE4 = 0x40,      /**< Module is transmitting Data Nibble 4 */
        SENT_TRANSMIT_NIBBLE5 = 0x50,      /**< Module is transmitting Data Nibble 5 */
        SENT_TRANSMIT_NIBBLE6 = 0x60,      /**< Module is transmitting Data Nibble 6 */
        SENT_TRANSMIT_CRC     = 0x70,      /**< Module is transmitting Data CRC */
        SENT_TRANSMIT_PAUSEPERIOD = 0x80   /**< Indicates whether the module is transmitting a Pause period */

    }SENT_TRANSMIT_STATUS;

## Summary

Defines the SENT transmit status.

## Description

This enum defines the SENT transmit status. More than one of these values may be OR'd together to create a complete status value. To test a value of this type, the bit of interest must be AND'ed with value and checked to see if the result is non-zero.

## Remarks

None.