Jump to main content

##

# 2.73.50 NVMCTRL_INTERRUPT0_SOURCE Enum

## C

    typedef enum
    {
        NVMCTRL_INT_DONE = NVMCTRL_INTENCLR_DONE_Msk,
        NVMCTRL_INT_ADDRE = NVMCTRL_INTENCLR_ADDRE_Msk,
        NVMCTRL_INT_PROGE = NVMCTRL_INTENCLR_PROGE_Msk,
        NVMCTRL_INT_LOCKE = NVMCTRL_INTENCLR_LOCKE_Msk,
        NVMCTRL_INT_ECCSE = NVMCTRL_INTENCLR_ECCSE_Msk,
        NVMCTRL_INT_ECCDE = NVMCTRL_INTENCLR_ECCDE_Msk,
        NVMCTRL_INT_NVME = NVMCTRL_INTENCLR_NVME_Msk,
        NVMCTRL_INT_SUSP = NVMCTRL_INTENCLR_SUSP_Msk
    } NVMCTRL_INTERRUPT0_SOURCE;

## Summary

Defines the Interrupt sources for the main flash.

## Description

This enumeration defines the Interrupt sources for the main flash.

## Remarks

None.