Jump to main content

##

# 2.99.46 RTC_Timer16TimeStampGet Function

## C

    uint16_t RTC_Timer16TimeStampGet( void )

## Summary

Get the Time stamp of Tamper Detection.

## Description

This function is used to get the 32-bit counter Value at which the tamper Detection took place.

## Precondition

Tamper channels must be configured properly using MCC.

## Parameters

None.

## Returns

16-bit counter Value.

## Example

    uint16_t tamperTime = RTC_Timer16TimeStampGet();

## Remarks

This Feature may not be available on all devices. Refer to device Datasheet for more information..