Jump to main content

##

# 2.42.9 EIC_PinDebounceStateGet Function

## C

    bool EIC_PinDebounceStateGet ( EIC_PIN pin )

## Summary

Gets the De-bounce state of the EIC Pin.

## Description

This function gets the De-bounced state of the EIC Pin.

## Precondition

EIC_Initialize() must have been called first for the associated instance. The debounce feature should have been enabled in MCC on the desired pin.

## Parameters

Param | Description
--- | ---
pin | EIC Pin number

## Returns

True, If the EIC Pin De-bounce state is set and False otherwise.

## Example

    if (true == EIC_PinDebounceStateGet(EIC_PIN_3))
    {
        // The pin was debounced and the state of the pin is logic high.
    }

## Remarks

None.