Jump to main content

##

# 2.81.21 PIO_PinInterruptDisable Function

## C

    void PIO_PinInterruptDisable(PIO_PIN pin)

## Summary

Disables IO interrupt on selected IO pin.

## Description

This function disables IO interrupt on selected IO pin.

## Precondition

Corresponding pin must be configured in interrupt mode in MCC Pin Manager. PIO_Initialize() must have been called.

## Parameters

Param | Description
--- | ---
pin | One of the IO pins from the enum PIO_PIN

## Returns

None.

## Example

    PIO_PinInterruptDisable(PIO_PIN_PB3);

## Remarks

None.