Jump to main content

##

# 2.38.14 EC_REG_BANK_VTRxPadMonOverrideProtEn Function

## C

    /* x = VTR PAD monitor number */

    void EC_REG_BANK_VTRxPadMonOverrideProtEn(void)

## Summary

When PAD monitor override feature is enabled calling this API powers off the input and output buffers and a weak pulldown is applied

## Description

When PAD monitor override feature is enabled calling this API powers off the input and output buffers and a weak pulldown is applied

## Precondition

None

## Parameters

None

## Returns

None

## Example

    EC_REG_BANK_VTR1PadMonOverrideProtEn();

## Remarks

None