Jump to main content

##

# 2.92.18 QMSPI_XFER_T Struct

## C

    typedef struct
    {
        /* Command */
        uint8_t command;
        /* Address Enable */
        bool address_enable;
        /* 32-bit Address Enable */
        bool address_32_bit_en;
        /* Address */
        uint32_t address;
        /* Dummy Byte */
        uint8_t num_of_dummy_byte;
        /* QMSPI Mode */
        QMSPI_INTERFACE_MODE qmspi_ifc_mode;
    } QMSPI_XFER_T;

## Summary

Defines the data type for the QMSPI transfer.

## Description

This data type should be used for QMSPI command/register transfer.

## Remarks

None.