Jump to main content

##

# 2.131.49 USART_STOP_BIT Enum

## C

    /* Blocking, non-blocking and ring buffer mode */

    typedef enum
    {
        USART_STOP_1_BIT = US_MR_USART_NBSTOP_1_BIT,
        USART_STOP_1_5_BIT = US_MR_USART_NBSTOP_1_5_BIT,
        USART_STOP_2_BIT = US_MR_USART_NBSTOP_2_BIT,

        /* Force the compiler to reserve 32-bit memory for each enum */
        USART_STOP_INVALID = 0xFFFFFFFF

    } USART_STOP;

## Summary

Defines the length of stop bits.

## Description

This may be in the USRTx_SerialSetup API to change the UART stop bits configuration

## Remarks

None.