Jump to main content

##

# 2.95.2 RCON_ResetCauseClear Function

## C

    void RCON_ResetCauseClear( RCON_RESET_CAUSE cause )

## Summary

Clears the particular reset cause status bit.

## Description

This function clears the particular reset bit in the RCON register. Multiple reasons for a reset can be ORed together and given as an input parameter to clear them simultaneously.

## Precondition

None.

## Parameters

Param | Description
--- | ---
cause | Reset status needs to be clear

## Returns

None.

## Example

    RCON_ResetCauseClear( RCON_RESET_CAUSE_POR | RCON_RESET_CAUSE_BOR );

## Remarks

None.