Jump to main content

##

# 2.110.16 SERCOMx_USART_WriteByte Function

## C

    /* x = SERCOM instance number */

    /* Blocking mode */

    void SERCOMx_USART_WriteByte( int data )

## Summary

Submits a byte of data to the given USART peripheral to transfer

## Description

This function submits a byte of data to the USART peripheral to transfer. This Function is available only in non-interrupt mode.

## Precondition

SERCOMx_USART_Initialize must have been called for the associated USART instance.

## Parameters

Param | Description
--- | ---
data | Data byte to be transferred.

## Returns

None

## Example

    char myData = 'A';

    SERCOM0_USART_WriteByte(myData);

## Remarks

None