Jump to main content

##

# 2.73.8 NVMCTRL_ErrorGet Function

## C

The prototype of NVMCTRL_ErrorGet() varies based on device family. Refer to the generated header file for the actual prototype to be used.

    NVMCTRL_ERROR NVMCTRL_ErrorGet( void );

    uint16_t NVMCTRL_ErrorGet( void );

## Summary

Returns the error state of NVM controller.

## Description

This function returns the error status of the last NVMCTRL operation. The return value can be either None, a single error or a combination of multiple error conditions.

## Precondition

None.

## Parameters

None

## Returns

Return NVMCTRL_ERROR type of value. In case of error, this value can be a combination of multiple and different error conditions.

## Example

    uint16_t nvm_error = 0;

    nvm_error = NVMCTRL_ErrorGet();

## Remarks

None.