Jump to main content

##

# 2.33.10 DMT_StatusGet Function

## C

    uint32_t DMT_StatusGet( void )

## Summary

Returns status flag from the DMT Status Register.

## Description

This function reads and returns the current status of the DMT. The status value is a 32-bit number representing various status flags and conditions of the DMT.

## Precondition

The returned status value is the raw value from the DMT status register and may need to be interpreted based on the specific bits defined for the DMT status.

## Parameters

None

## Returns

Status value of DMT.

## Example

    uint32_t statusValue = 0;

    DMT_Enable();
    statusValue = DMT_StatusGet();

## Remarks

None