Jump to main content

##

# 2.130.32 UART_PARITY Enum

## C

    /* Blocking, non-blocking and ring buffer mode */

    The UART_PARITY enumerations vary based on the device family. Refer the generated header file for the actual UART_PARITY enumerator constants.

## Summary

Defines the type of parity for UART peripheral.

## Description

This may be in the UARTx_SerialSetup API to change the parity configuration

## Remarks

None