Jump to main content

##

# 3.32.12 OTP Memory Controller (OTPC)

OTP memory area is mapped into 32-bit words. Each 32-bit word is part of one packet. Each packet contains a 32-bit header and 32-bit words of payload(data). The number of payload words is defined in the header.

This mapping system allows three important functions for an OTP memory:

- Gives a flexible size for any type of data

- Improves the security by identifying and masking key areas to the System bus

- Provides an easy way to invalidate a packet and create a replacement packet (key, data) while free space is available in OTP

## Using The Library

OTPC plib supports the following activities on the user area of the OTP:

1. Create a new packet in the otp area with a given payload

2. Update the payload of an existing user packet

3. Read the payload associated with a packet

4. Lock the packet to prevent any further modification

5. Invalidate a packet to make sure that it is no longer used

6. Hide a packet to prevent reading its payload

## Library Interface

OTP Memory Controller peripheral library provides the following interfaces:

Functions

Name | Description
--- | ---
OTPC_Initialize | Initializes given OTPC instancee
OTPC_WritePacket | Perform an OTPC packet write
OTPC_UpdatePayload | Updates the payload of a packet
OTPC_ReadPacket | Reads a User packet from OTPC from a given address
OTPC_LockPacket | Locks the packet
OTPC_InvalidatePacket | Invalidates the packet
OTPC_HidePacket | Hides the packet

Data types and constants

Name | Type | Description
--- | --- | ---
OTPC_PACKET_TYPE | Enum | Identifies user area packet types
otpc_error_code_t | Enum | Identifies OTPC error codes
OTPC_NEW_PACKET | Struct | Structure identifying a new OTPC packet