Jump to main content

##

# 2.3.6 ADCx_ConversionStart Function

## C

    void ADCx_ConversionStart( void ); // x is instance of the peripheral and it is applicable only for devices having multiple instances of the peripheral.

## Summary

Starts the ADC conversion with the software trigger.

## Description

This function triggers the ADC conversion of the selected channel

## Precondition

ADCx_Initialize() function must have been called first for the associated instance.

## Parameters

None.

## Returns

None.

## Example

    ADC0_Initialize();
    ADC0_ConversionStart();

## Remarks

This function should be called for each conversion when SW trigger for conversion is selected.