Jump to main content

##

# 2.66.1 MCSPIx_Initialize Function

## C

    /* x = MCSPI instance number */

    /* MCSPI master and slave mode */
    void MCSPIx_Initialize (void)

## Summary

Initializes MCSPI module of the device

## Description

This function initializes MCSPI PLIB of the device with the values configured in MCC GUI. Once the peripheral is initialized, transfer APIs can be used to transfer the data.

## Precondition

MCC GUI should be configured with the right values.

## Parameters

None.

## Returns

None.

## Example

    MCSPI1_Initialize();

## Remarks

This function must be called only once and before any other MCSPI function is called.