Jump to main content

##

# 2.120.2.28 TCx_QuadratureInitialize Function

## C

    /* x = TC instance number */
    void TCx_QuadratureInitialize ( void );

## Summary

Initializes given instance of TC channel in quadrature mode.

## Description

This function initializes given instance of TC channel in quadrature mode with options configured in MCC GUI.

## Precondition

MCC GUI should be configured with the desired options.

## Parameters

None.

## Returns

None.

## Example

    TC0_QuadratureInitialize();

## Remarks

This function must be called before any other TC function is called. This function is normally called only be called once during system initialization.