Jump to main content

##

# 2.31.10 DMA_ChannelInterruptFlagsGet Function

## C

    DMA_INT DMA_ChannelInterruptFlagsGet ( DMA_CHANNEL channel )

## Summary

This API is used to get the DMA channel interrupt flags

## Description

This API is used to get the DMA channel interrupt flags

## Precondition

DMA should have been initialized by calling DMA_Initialize.

## Parameters

Param | Description
--- | ---
channel | DMA channel

## Returns

DMA_INT - Bit-wise OR of following interrupt flags. DMA_INT_START_DETECTED, DMA_INT_TRANSFER_ABORT, DMA_INT_CELL_TRANSFER_COMPLETE, DMA_INT_BLOCK_TRANSFER_COMPLETE, DMA_INT_BLOCK_HALF_TRANSFER_COMPLETE, DMA_INT_LINKED_LIST_DONE, DMA_INT_WRITE_ERROR, DMA_INT_READ_ERROR

## Example

    DMA_INT int_flag;

    int_flag = DMA_ChannelInterruptFlagsGet (DMA_CHANNEL_0);

## Remarks

None.