Jump to main content

##

# 2.115.2 SQIx_DMASetup Function

## C

    bool SQIx_DMASetup( void ); // x - Instance of the SQI peripheral

## Summary

Sets up SQI peripheral to DMA mode.

## Description

This function can be used to configure SQI peripheral to DMA mode at run-time.

## Precondition

SQIx_Initialize must have been called for the associated SQI instance.

## Parameters

None.

## Returns

None

## Example

    SQI1_DMASetup();