Jump to main content

##

# 2.62.9 LEDx_SegmentsStepSizeSet Function

## C

    /* x = LED peripheral instance number */

    void LEDx_SegmentsStepSizeSet(uint32_t stepSzVal)

## Summary

Configures the amount the current duty cycle is adjusted at the end of every PWM period

## Description

Configures the amount the current duty cycle is adjusted at the end of every PWM period

## Precondition

None

## Parameters

Param | Description
--- | ---
stepSzVal | Step size value, bitwise OR of all the steps

## Returns

None

## Example

    LED0_SegmentsStepSizeSet(0x87654321);

## Remarks

None