Jump to main content

##

# 2.127.8 TSENS_ConversionResultGet Function

## C

    uint32_t TSENS_ConversionResultGet(void);

## Summary

Returns the measured temperature value

## Description

This function returns the last measured temperature value.

## Precondition

TSENS_Initialize() function must have been called first for the associated instance

## Parameters

None

## Returns

result - 24-bit last measured temperature value

## Example

    uint32_t result;
    TSENS_Initialize();
    TSENS_Enable();
    TSENS_ConversionStart();
    while(!TSENS_ConversionStatusGet());
    result = TSENS_COnversionResultGet();

## Remarks

This function can be called from interrupt or by polling the status when result is available. The result is 24-bit value in two's complement format.