Jump to main content

##

# 2.18.2 CMPx_DACDataWrite Function

## C

    // x is the instance number of the CMP peripheral
    inline static void CMPx_DACDataWrite(size_t value);

## Summary

Writes DAC data to register.

## Description

This function writes DAC data to register.

## Precondition

None.

## Parameters

Param | Description
value | DAC Data write value

## Returns

None.

## Example

    CMP1_DACDataWrite(value);

## Remarks

Available only in DC mode.