Jump to main content

##

# 2.62.7 LEDx_LowDelaySet Function

## C

    /* x = LED peripheral instance number */

    void LEDx_LowDelaySet(uint16_t ld)

## Summary

Specifies the number of PWM periods to wait before updating the current duty cycle when the current duty cycle is greater than or equal to the value MIN in register LED_LIMIT

## Description

Specifies the number of PWM periods to wait before updating the current duty cycle when the current duty cycle is greater than or equal to the value MIN in register LED_LIMIT

## Precondition

None

## Parameters

Param | Description
--- | ---
ld | low delay value

## Returns

None

## Example

    LED0_LowDelaySet(10);

## Remarks

None